Removed Pin From Net: NetName=NetC14_2 Pin=R15-1
Removed Pin From Net: NetName=NetD1_1 Pin=R15-2
Removed Pin From Net: NetName=NetIC1_5 Pin=R18-1
Removed Pin From Net: NetName=NetC5_1 Pin=R18-2
Removed Member From Class: ClassName=VIPer31 flyback iso PSR-SSR Member=R15
Removed Member From Class: ClassName=VIPer31 flyback iso PSR-SSR Member=R18
Change Component Footprint: Designator=C3 Old Footprint=CAPOL-7.5X16 New Footprint=CAPOL-5X12.5
Change Component Footprint: Designator=C4 Old Footprint=CAPOL-7.5X16 New Footprint=CAPOL-5X12.5
Change Component Footprint: Designator=Rz Old Footprint=R-0603-B2 New Footprint=R-0805-B2
Change Component Footprint: Designator=D2 Old Footprint=SMB-2 New Footprint=D2PAK
Change Component Comment : Designator=Dz Old Comment=18V New Comment=22
Change Component Comment : Designator=Rz Old Comment=47R New Comment=12R
Change component parameters: Designator = "R10"; Footprint = "R-0603-B2"; UniqueID = "\WSKEPWBM"
Change component parameters. Clean all parameters for all variants
Change component parameters (AddParameter): Name = "Distributor"; Value = "RS"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Distributor code"; Value = "679-0415"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Package"; Value = "SMD 0603"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Part number"; Value = "CRCW0603470KFKEA"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Supplier"; Value = "Vishay"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Value"; Value = "470kO ±1%, 0.1W"; VariantName = "[No Variations]"
Change component parameters: Designator = "R11"; Footprint = "R-0603-B2"; UniqueID = "\IFNSBGFJ"
Change component parameters. Clean all parameters for all variants
Change component parameters (AddParameter): Name = "Distributor"; Value = "RS"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Distributor code"; Value = "679-0005"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Package"; Value = "SMD 0603"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Part number"; Value = "CRCW060322K0FKEA"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Supplier"; Value = "Vishay"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Value"; Value = "22KO ±1%, 0.1W"; VariantName = "[No Variations]"
Change component parameters: Designator = "R12"; Footprint = "R-0603-B2"; UniqueID = "\EUFIGOFF"
Change component parameters. Clean all parameters for all variants
Change component parameters (AddParameter): Name = "Distributor"; Value = "RS"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Distributor code"; Value = "678-9746"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Package"; Value = "SMD 0603"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Part number"; Value = "CRCW0603130KFKEA"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Supplier"; Value = "Vishay"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Value"; Value = "130 kO ±1%, 0.1 W"; VariantName = "[No Variations]"
Change component parameters: Designator = "R13"; Footprint = "R-0603-B2"; UniqueID = "\OMGVEEAQ"
Change component parameters. Clean all parameters for all variants
Change component parameters (AddParameter): Name = "Distributor"; Value = "RS"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Distributor code"; Value = "213-2430"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Package"; Value = "SMD 0603"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Part number"; Value = "CRG0603F15K"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Supplier"; Value = "TE Connectivity"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Value"; Value = "15 kO ±1%, 0.1W, 0603"; VariantName = "[No Variations]"
Change component parameters: Designator = "R16"; Footprint = "R-0603-B2"; UniqueID = "\LNYASSMO"
Change component parameters. Clean all parameters for all variants
Change component parameters (AddParameter): Name = "Distributor"; Value = "RS"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Distributor code"; Value = "679-0419"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Package"; Value = "SMD 0603"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Part number"; Value = "CRCW0603470RFKEA"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Supplier"; Value = "Vishay"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Value"; Value = "470O ±1%, 0.1W"; VariantName = "[No Variations]"
Change component parameters: Designator = "Rz"; Footprint = "R-0805-B2"; UniqueID = "\XLJUGKIK"
Change component parameters. Clean all parameters for all variants
Change component parameters (AddParameter): Name = "Distributor"; Value = "RS"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Distributor code"; Value = "223-0253"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Package"; Value = "SMD 0805"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Part number"; Value = "CRG0805F47R"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Supplier"; Value = "TE Connectivity"; VariantName = "[No Variations]"
Change component parameters (AddParameter): Name = "Value"; Value = "47O ±1%, 0.125W"; VariantName = "[No Variations]"
Added Component: Designator=L3(R-0805-B)
Add component. Clean all parameters for all variants
Add component (AddParameter): Name = "Distributor"; Value = "Digikey"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Distributor code"; Value = "732-10755-1-ND"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Package"; Value = "Lu x La: 0,157 x 0,157" (4,00 x 4,00 mm)"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Part number"; Value = "74404043033A"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Supplier"; Value = "Wurth Electronics Inc"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Value"; Value = "3.3UH 3.23A 33 MOHM"; VariantName = "[No Variations]"
Added Pin To Net: NetName=NetD1_1 Pin=L3-1
Added Pin To Net: NetName=NetC14_2 Pin=L3-2
Added Member To Class: ClassName=VIPer31 flyback iso PSR-SSR Member=Component L3 10uH
Added Room: Name=VIPer31 flyback iso PSR-SSR
